DEPARTMENT OF TRANSPORTATION

Federal Aviation Administration

14 CFR Part 39 [62 FR 38898 No. 139, 7/21/97]	Raytheon Aircraft
   Company (Beech)

Amendment 39-10073
Recurring: No

[Docket No. 96-CE-34-AD; Amendment 39-10073; AD 97-14-15]
RIN 2120-AA64
 
Airworthiness Directives; Raytheon Aircraft Company (Formerly Known as Beech Aircraft Corporation) Models E33, F33, G33, E33A, F33A, E33C, F33C, C35, D35, E35, F35, G35, H35, J35, K35, M35, N35, P35, S35, V35, V35A, V35B, V35TC, V35ATC, V35BTC, 36, A36, A36TC, B36TC, 50, B50, C50, 95-55, 95A55, 95B55, 95C55, D55, E55, 56TC, A56TC, 58, 58TC, 95, B95, B95A, D95A, and E95 Airplanes

AGENCY: Federal Aviation Administration, DOT.

ACTION: Final rule.

SUMMARY: This amendment adopts a new airworthiness directive (AD) that applies to Raytheon Aircraft Company (formerly known as Beech Aircraft Corporation) Models E33, F33, G33, E33A, F33A, E33C, F33C, C35, D35, E35, F35, G35, H35, J35, K35, M35, N35, P35, S35, V35, V35A, V35B, V35TC, V35ATC, V35BTC, 36, A36, A36TC, B36TC, 50, B50, C50, 95-55, 95A55, 95B55, 95C55, D55, E55, 56TC, A56TC, 58, 58TC, 95, B95, B95A, D95A, and E95 airplanes. This action requires checking the cabin side door handle and the utility door handle from the interior of the airplane for proper locking. If the door handles do not lock, the proposed AD would require reinstalling the door handles correctly for the lock to engage. Nine reports of the utility and cabin door handle opening from the interior of the airplane without depressing the lock release button prompted this action. The actions specified by this AD are intended to prevent unintentional opening of the cabin side door and the utility door from the interior of the airplane, which, if not detected and corrected, could result in loss of control of the airplane.

DATES: Effective September 2, 1997.
	The incorporation by reference of certain publications listed in the regulations is approved by the Director of the Federal Register as of September 2, 1997.

ADDRESSES: Service information that applies to this AD may be obtained from Raytheon Aircraft Company, P.O. Box 85, Wichita, Kansas 67201-0085. This information may also be examined at the Federal Aviation Administration (FAA), Central Region, Office of the Assistant Chief Counsel, Attention: Rules Docket 96-CE-34-AD, Room 1558, 601 E. 12th Street, Kansas City, Missouri 64106; or at the Office of the Federal Register, 800 North Capitol Street, NW., Suite 700, Washington, DC.

FOR FURTHER INFORMATION CONTACT: Larry Engler, Aerospace Engineer, FAA, Wichita Aircraft Certification Office, 1801 Airport Rd., Rm. 100, Mid-Continent Airport, Wichita, Kansas 67209; telephone (316) 946-4122; facsimile (316) 946-4407.

SUPPLEMENTARY INFORMATION:

Events Leading to the Issuance of This AD

	A proposal to amend part 39 of the Federal Aviation Regulations (14 CFR part 39) to include an AD that would apply to Raytheon Aircraft Company (Raytheon) (formerly known as Beech Aircraft Corporation) Models E33, F33, G33, E33A, F33A, E33C, F33C, C35, D35, E35, F35, G35, H35, J35, K35, M35, N35, P35, S35, V35, V35A, V35B, V35TC, V35ATC, V35BTC, 36, A36, A36TC, B36TC, 50, B50, C50, 95-55, 95A55, 95B55, 95C55, D55, E55, 56TC, A56TC, 58, 58TC, 95, B95, B95A, D95A, and E95 airplanes was published in the Federal Register on December 23, 1996 (61 FR 67505). The action proposed to require checking the cabin side door and the utility door handle from the interior of the airplane for proper locking. If the handles do not lock, this action proposed to require procedures for re-installing the door handles correctly for the lock to engage. Accomplishment of the proposed action would be in accordance with Raytheon Aircraft Mandatory Service Bulletin No. 2693, Issued: May, 1996.
	Interested persons have been afforded an opportunity to participate in the making of this amendment. Due consideration has been given to comments received from three different commenters.

Comment 1: No Need for AD Action

	The first commenter states that the use of the words "may result" or "could occur" in the section titled "Events Leading to the Proposed Action" of the preamble indicates that there have been no actual incidents or accidents because of the improperly installed door handle and there is no need for the AD action.
	The FAA does not concur that there is no need for AD action. The FAA uses the phrases "may result" and "could occur" to emphasize the possibility of another incident or accident occurring based on the history and reports of incidents and accidents that have already occurred. The AD preamble is used to describe what the FAA knows has already happened and to justify the possible consequences if the affected airplane operators do not comply with the AD action. The notice of proposed rulemaking (NPRM) did not specify the number of occurrences reported on these cabin door handles. There have been nine reports of these door handles not locking properly.
	No changes have been made to the final rule as a result of this comment.

Comment 2: No Incidents, Only Reports

	The same commenter also states that the phrase "incidents described above" in the section titled "Explanation of the Provisions of the Proposed Action" makes reference to incidents described in the preamble and there are no incidents described, but only reports of improperly installed door handles.
	The FAA concurs and will change all incident references in the final rule to reports.

Comment 3: Cost Impact

	A commenter states that the cost of repetitive inspections and the owners/operators time for the burdensome paperwork that is required to comply with an AD is not figured into the cost of the proposed AD.
	The FAA concurs, but states that the cost of the repetitive inspections is not figured into the cost impact per airplane or for the entire U.S. fleet because there are no repetitive inspections proposed in the NPRM. Likewise, the FAA does not estimate the time for paperwork to comply with the proposed AD because the FAA has no reasonable means of obtaining this information.
	No changes have been made to the final rule as a result of this comment.

Comment 4: Include Subsequent Service Bulletin Revisions in AD

	A commenter states that the AD compliance should not only specify that the proposed action be accomplished in accordance with Raytheon Service Bulletin (SB) No. 2693, dated May, 1996, but also include any subsequent revisions to the referenced service bulletin.
	The FAA does not concur. The FAA cannot approve data that does not exist. Approval of this nature could adversely affect aviation safety if modifications were included in the subsequent service bulletins that did not carry normal FAA review.
	No changes have been made to the final rule as a result of this comment.

Comment 5: Improper Installation Is Not Justification for an AD

	One commenter explains that AD's normally do not address a potential problem based on an improperly installed part. The commenter states that if AD's were issued on this basis alone, why doesn't the FAA issue AD's to cover the installation of all aircraft parts?
	FAA does not concur with this commenter's statement. The NPRM is written because the information provided in the maintenance manual does not cover the re-installation of the door handle, once removed. The NPRM provides the information needed to assure that the door handles are re-installed correctly. The FAA will add a Note in the AD recommending that reference be made to the service bulletin in the maintenance manual.

Comment 6: No Interior Cabin or Utility Doors

	A commenter states that a revision is needed in the "Summary" to correctly identify the area to be inspected. As written, the phrase "* * *interior cabin side door handle and interior utility door handle* * *" leads the reader to believe there are interior doors on the airplane. There are no interior cabin side doors or interior utility doors.
	The FAA concurs and has re-written the "Summary" to correctly describe the doors as "* * *cabin side door handle and utility door handle from the interior of the airplane * * *" for better clarification.

Comment 7: Unsafe Condition Not Defined Correctly

	One commenter states that the phrase "* * * while in flight * * * could result in injury to passengers * * *" is misleading. The commenter states that the airloads on the door after rotation of the airplane should prevent the door from opening, and the only potential for injury is during taxi operations.
	The FAA concurs with this statement. After further review of the reports made, the FAA has determined that no injuries have occurred from the door coming ajar. As a result, the FAA has changed the statements referring to passenger injury during flight or during taxi operations. Instead, the statement has been changed to "* * * could result in loss of control of the airplane." The reason for this change is that loss of control of the airplane could result from either a startled passenger grabbing an airplane control should the door come ajar because the door handle lock didn't lock, or the pilot having to lean over and shut the door because a passenger inadvertently leaned on the door handle causing it to come ajar.

Comment 8: Doors Were Installed Correctly at Factory

	A commenter states that this problem was discovered in the field as a result of removing the door handle and re-installing the handle incorrectly, and the door handles were not installed at the factory incorrectly.
	The FAA concurs and has made an effort to clarify the cause of the problem, so as not to imply that the manufacturer is at fault.
	No changes were made as a result of this comment.

Comment 9: Change in Compliance Time

	Another commenter states that a change should be made to the compliance time of the AD. The commenter wants to eliminate the phrase "* * * whichever occurs first,* * *" because this implies that the door handle only needs to be checked and corrected one time. The commenter states that repetitive checks are needed to the door handle when removed in the future, and incorrectly re-installed.
	The FAA does not concur that the phrase "* * * whichever occurs first,* * *" is unnecessary. The purpose for this phrase is to make sure the door handles are checked at the first possible opportunity. This means the operator has 50 hours time-in-service (TIS) to check the door handles, but if the door handles are removed prior to the expiration of that time, the operators must check the door handles and verify that they are locking correctly and does not have to check the door handles at the expiration of 50 hours TIS after the effective date of the AD.
	The FAA is not requiring a repetitive check because the purpose of this AD is to have the entire fleet check the door handles to make sure they are locking correctly. If the door handles are not locking, then the operator should have the door handles re-installed to lock correctly. After the initial check to assure every affected airplane has locking door handles, the FAA is relying on regular maintenance to catch this problem. The FAA will add a Note recommending that reference be made to the service bulletin in the maintenance manual.

Comment 10: Certified/Licensed Versus Certificated

	All three commenters state that airframe mechanics and pilots are not "licensed" or "certified", but are "certificated." The FAA concurs and has changed all references to "licensed airframe mechanics" or "certified pilots" in the preamble and the AD to read "certificated airframe mechanics" or "certificated pilots."

The FAA's Determination

	After careful review of all available information related to the subject presented above, the FAA has determined that air safety and the public interest require the adoption of the rule as proposed except editorial corrections mentioned above. The FAA has determined that these corrections will not change the meaning of the AD and will not add any additional burden upon the public than was already proposed.

Cost Impact

	The FAA estimates that 19,000 airplanes in the U.S. registry will be affected by this AD, that it will take approximately 1 workhour per airplane to accomplish the required initial check and there is no labor cost because the check may be performed by the owner/operator holding at least a private pilot certificate as authorized by Sec. 43.7 of the Federal Aviation Regulations (14 CFR 43.7), and must be entered into the aircraft records showing compliance with this AD in accordance with Sec. 43.11 of the Federal Aviation Regulations (14 CFR 43.11). Based on these figures, there is no initial cost impact of this AD on U.S. operators. This figure is based upon the assumption that no affected airplane owner/operator has accomplished this check. The FAA has no way of determining the number of owners/operators who may have already accomplished this action.

Regulatory Impact

	The regulations adopted herein will not have substantial direct effects on the States, on the relationship between the national government and the States, or on the distribution of power and responsibilities among the various levels of government. Therefore, in accordance with Executive Order 12612, it is determined that this final rule does not have sufficient federalism implications to warrant the preparation of a Federalism Assessment.
	For the reasons discussed above, I certify that this action (1) is not a "significant regulatory action" under Executive Order 12866; (2) is not a "significant rule" under DOT Regulatory Policies and Procedures (44 FR 11034, February 26, 1979); and (3) will not have a significant economic impact, positive or negative, on a substantial number of small entities under the criteria of the Regulatory Flexibility Act. A copy of the final evaluation prepared for this action is contained in the Rules Docket. A copy of it may be obtained by contacting the Rules Docket at the location provided under the caption ADDRESSES.

List of Subjects in 14 CFR Part 39

	Air transportation, Aircraft, Aviation safety, Incorporation by reference, Safety.

Adoption of the Amendment

	Accordingly, pursuant to the authority delegated to me by the Administrator, the Federal Aviation Administration amends part 39 of the Federal Aviation Regulations (14 CFR part 39) as follows:

PART 39--AIRWORTHINESS DIRECTIVES

	1. The authority citation for part 39 continues to read as follows:

	Authority: 49 USC 106(g), 40113, 44701.

Sec. 39.13  [Amended]

	2. Section 39.13 is amended by adding a new airworthiness directive (AD) to read as follows:

97-14-15  RAYTHEON AIRCRAFT COMPANY: Amendment 39-10073; 
Docket No. 96-CE-34-AD.

	Applicability: Models E33, F33, G33, E33A, F33A, E33C, F33C, C35, D35, E35, F35, G35, H35, J35, K35, M35, N35, P35, S35, V35, V35A, V35B, V35TC, V35ATC, V35BTC, 36, A36, A36TC, B36TC, 50, B50, C50, 95-55, 95A55, 95B55, 95C55, D55, E55, 56TC, A56TC, 58, 58TC, 95, B95, B95A, D95A, and E95 airplanes (all serial numbers), certificated in any category.

	Note 1: This AD applies to each airplane identified in the preceding applicability provision, regardless of whether it has been modified, altered, or repaired in the area subject to the requirements of this AD. For airplanes that have been modified, altered, or repaired so that the performance of the requirements of this AD is affected, the owner/operator must request approval for an alternative method of compliance in accordance with paragraph (d) of this AD. The request should include an assessment of the effect of the modification, alteration, or repair on the unsafe condition addressed by this AD; and, if the unsafe condition has not been eliminated, the request should include specific proposed actions to address it.

	Compliance: Required within the next 50 hours time-in-service (TIS) after the effective date of this AD or at the next door handle removal after the effective date of this AD, whichever occurs first, unless already accomplished.

	To prevent unintentional opening of the cabin side door and the utility door from the interior of the airplane, which if not detected and corrected, could result in loss of control of the airplane, accomplish the following:
   (a)	Check the cabin side door handle and the utility door handle from the interior of the airplane for proper locking (rotating the door handle clockwise without depressing the lock release button) in accordance with the Accomplishment Instructions section of Raytheon Service Bulletin (SB) No. 2693, Issued May, 1996.
	(1)	If the door handle opens the door when rotated, without depressing the handle's lock release button, prior to further flight, correct the door handle lock by removing the door handle, and re-installing the door handle so that the lock release button locks the door in accordance with the Accomplishment Instructions section in Raytheon SB No. 2693, Issued May, 1996.
	(2)	If the door handle is locked and will only unlock by depressing the handle door lock release button, then no further action is necessary.

	Note 2: The FAA strongly recommends entering a reference to Raytheon SB No. 2693, Issued May, 1996 into the applicable airplane maintenance manual.

   (b)	The check required in paragraph (a) of this AD may be performed by the owner/operator holding at least a private pilot certificate as authorized by section 43.7 of the Federal Aviation Regulations (14 CFR 43.7), and must be entered into the aircraft records showing compliance with this AD in accordance with section 43.11 of the Federal Aviation Regulations (14 CFR 43.11).
   (c)	Special flight permits may be issued in accordance with sections 21.197 and 21.199 of the Federal Aviation Regulations (14 CFR 21.197 and 21.199) to operate the airplane to a location where the requirements of this AD can be accomplished.
   (d)	An alternative method of compliance or adjustment of the compliance time that provides an equivalent level of safety may be approved by the Manager, Wichita Aircraft Certification Office, 1801 Airport Rd., Rm. 100, Mid-Continent Airport, Wichita, Kansas 67209. The request shall be forwarded through an appropriate FAA Maintenance Inspector, who may add comments and then send it to the Manager, Wichita Aircraft Certification Office.

	Note 3: Information concerning the existence of approved alternative methods of compliance with this AD, if any, may be obtained from the Wichita Aircraft Certification Office.

   (e)	The check and re-installation required by this AD shall be done in accordance with Raytheon Aircraft Mandatory Service Bulletin No. 2693, Issued: May, 1996. This incorporation by reference was approved by the Director of the Federal Register in accordance with 5 U.S.C. 552(a) and 1 CFR part 51. Copies may be obtained from Raytheon Aircraft Company, P. O. Box 85, Wichita, Kansas 67201-0085. Copies may be inspected at the FAA, Central Region, Office of the Assistant Chief Counsel, Room 1558, 601 E. 12th Street, Kansas City, Missouri, or at the Office of the Federal Register, 800 North Capitol Street, NW., Suite 700, Washington, DC.
   (f)	This amendment (39-10073) becomes effective on September 2, 1997.

	Issued in Kansas City, Missouri, on July 2, 1997.

James E. Jackson, Acting Manager, Small Airplane Directorate, Aircraft Certification Service.

FOR FURTHER INFORMATION CONTACT: Larry Engler, Aerospace Engineer, FAA, Wichita Aircraft Certification Office, 1801 Airport Rd., Rm. 100, Mid-Continent Airport, Wichita, Kansas 67209; telephone (316) 946-4122; facsimile (316) 946-4407.

Manufacturer's Service Information: Included Below.
Raytheon Aircraft Mandatory Service Bulletin No. 2693

Copies may be obtained from Raytheon Aircraft Company, P. O. Box 85, Wichita, 
Kansas 67201-0085.

RAYTHEON AIRCRAFT
MANDATORY SERVICE BULLETIN NO. 2693
Beech Models 33, 35, 36, 50, 55, 56 58, 95
ATA Code 52-10
Recurring Inspection
ISSUED: May, 1996
SUBJECT: DOORS - INSPECTION OF THE INTERIOR DOOR HANDLES

REASON:
This Service Bulletin is being issued to inspect the interior cabin door handle and the interior utility door handle for proper installation. An investigation into a report that the utility door opened without having to depress the handle lock release button has revealed that if the door handle is not properly oriented during installation, the handle lock mechanism does not restrict inadvertent unlatching of the door.

EFFECTIVITY:
CIVIL AIRPLANES
BEECH Bonanza Models E33, F33, G33, E33A, F33A, E33C, and F33C, all serials:
Bonanza Models C35, D35, E35, F35, G35, H35, J35, K35, M35, N35, P35, S35, V35, V35A, V35B, V35TC, V35ATC, and V35BTC, all serials;
Bonanza Models 36, A36, A36TC, and B36TC, all serials;
Twin Bonanza Models 50, B50, and C50, all serials;
Baron Models 95-55, 95A55, 95B55, 95C55, D55, and E55, all serials;
Baron Models 56TC and A56TC, all serials;
Baron Models 58 and 58TC, all serials;
Travel Air Models 95, B95, B95A, D95A, and E95, all serials.
MILITARY AIRPLANES
Models L23A and L23B, all serials;
Model 95B55B, all serials.

COMPLIANCE:
Raytheon Aircraft Company considers this to be a Mandatory Service Bulletin which must be accomplished prior to next flight and any time the interior door handle is removed.
The inspection portion may be accomplished by a certified pilot. If the inspection discloses that the interior door handle is not operating properly, take the airplane to the nearest appropriate service center for repairs.
An Airworthiness Directive has been requested on the matter covered by this Service Bulletin.

APPROVAL:
Engineering data contained in this Service Bulletin is FAA Approved.

MANPOWER:
The following information is for planning purposes only:
Estimated man-hours for inspection: .5 hour.
Estimated man-hours for removal/orientation: 1 hour.
Suggested number of men: 1 man.
The above is an estimate based on experienced, properly equipped personnel complying with this Service Bulletin. Occasionally, after work has started, conditions may be found which could result in additional man-hours.

MATERIAL:
None.

SPARES AFFECTED:
None.

WARRANTY CREDIT:
None.

SPECIAL TOOLS:
None.

WEIGHT AND BALANCE:
None.

PUBLICATIONS AFFECTED:
It is recommended that a note "See Service Bulletin No. 2693" be made in the applicable airplane maintenance manual, Chapter 52.

ACCOMPLISHMENT INSTRUCTIONS:
This Service Bulletin shall be accomplished as follows:

INSPECTION OF THE INTERIOR CABIN DOOR HANDLE
   1.	Close and latch the cabin door.
   CAUTION
Rotation of the interior door handle without depressing the handle lock release button should not result in unlatching of the door.
   2.	Rotate the interior cabin door handle clockwise without depressing the handle lock release button.
	a.	If the door remains latched, no additional work is required for the cabin door handle.
	b.	If the door becomes unlatched, proceed to step 3.
   3.	Examine the handle lock release button for proper operation.
   NOTE
Depressing the handle lock release button should permit the handle to travel beyond the step in the base plate. When the handle lock release button is not depressed, the step should restrict handle travel to the open position.
	a.	If the interior door handle is in good operating condition, perform the REMOVAL/ORIENTATION OF THE INTERIOR DOOR HANDLE procedure provided in this Service Bulletin.
	b.	If the handle lock release button is not operating properly, perform the REMOVAL/ORIENTATION OF THE INTERIOR DOOR HANDLE procedure using a new handle.

INSPECTION OF THE INTERIOR UTILITY DOOR HANDLE
(FOR MODELS 36, A36, A36TC, B36TC, 58 AND 58TC ONLY)
   1.	Close and latch the utility door.
   CAUTION
Rotation of the interior door handle without depressing the handle lock release button should not result in unlatching of the door.
   2.	Rotate the interior utility door handle clockwise without depressing the handle lock release button.
	a.	If the door remains latched, no additional work is required for the utility door handle.
	b.	If the door becomes unlatched, proceed to step 3.
   3.	Examine the handle lock release button for proper operation.
   NOTE
Depressing the handle lock release button should permit the handle to travel beyond the step in the base plate. When the handle lock release button is not depressed, the step should restrict handle travel to the open position.
	a.	If the interior door handle is in good operating condition, perform the REMOVAL/ORIENTATION OF THE INTERIOR DOOR HANDLE procedure provided in this Service Bulletin.
 	b.	If the handle lock release button is not operating properly, perform the REMOVAL/ORIENTATION OF THE INTERIOR DOOR HANDLE procedure using a new handle.

REMOVAL/ORIENTATION OF THE INTERIOR DOOR HANDLE
   NOTE
It may be necessary to place the door handle in the unlatched position to access both screws used to secure the door handle.
   1.	Remove the two screws which secure the interior door handle base plate.
   2.	Slide the interior door handle from the shaft, maintaining the same orientation of the door handle with respect to the shaft.
   3.	Rotate the door handle 90 degrees clockwise, maintaining the base plate in the same position. Figure 1 illustrates the incorrect installation and correct installation of the interior door handles. (NOTE: Handle configuration of some airplanes may differ from what is shown in Figure 1).
   4.	Slide the interior door handle over the shaft and secure, using the screws removed in step 1.
   5.	Latch the door by rotating the interior door handle counterclockwise.
   CAUTION
Rotation of the interior door handle without depressing the handle lock release button should not result in unlatching of the door.
   6.	Rotate the interior door handle clockwise without depressing the handle lock release button. If the door remains latched, proceed to step 7. If the door becomes unlatched, repeat steps 1 through 6.
   7.	With the door latched, depress the handle lock release button while rotating the handle clockwise. Rotating the door handle clockwise while depressing the handle lock release button should unlatch the door.

RECORD COMPLIANCE:
The certified pilot should make an entry in the airplane log book reflecting satisfactory accomplishment of the inspection portion of this Service Bulletin. If the results of the inspection are not satisfactory, the mechanic should make an appropriate airframe log book entry reflecting repair.
   NOTE
If you are no longer in possession of this airplane, please forward this information to the present owner.
FIGURE 1
Raytheon Aircraft Company (RAC) issues Service information for the benefit of owners and fixed based operators in the form of two classes of Service Bulletins. The first class, Mandatory Service Bulletins (red border) includes changes, inspections and modifications that could affect safety or crashworthiness. RAC considers compliance with these Service Bulletins to be mandatory. RAC also issues Service Bulletins with no border which are designated as either recommended or optional in the compliance section within the bulletin. In the case of recommended Service Bulletins, RAC feels the changes, modifications, improvements or inspections will benefit the owner/operator and although highly recommended, Recommended Service Bulletins are not considered mandatory at the time of issuance. In the case of optional Service Bulletins, compliance with the changes, modifications, improvements or inspections is at the owner/operator's discretion. Both classes are mailed to:
   (a)	RAC Authorized Service Center.
   (b)	Owners of record on the FAA Aircraft Registration Branch List and the RAC International Owner Notification Service List.
   (c)	Those having a publications subscription.
Information on Owner Notification Service or subscriptions can be obtained though any RAC Authorized Service Center. As Mandatory Service Bulletins and Service Bulletins are issued, temporary notification in the Service Bulletin Master Index should be made until the index is revised. Warranty will be allowed only when specifically defined in the Service Bulletin and in accordance with the RAC Warranty Policy.
Unless otherwise designated, RAC Mandatory Service Bulletins, Service Bulletins and RAC Kits are approved for installation on RAC airplanes in original or RAC modified configurations only. RAC Mandatory Service Bulletins, Service Bulletins and Kits may not be compatible with airplanes modified by STC installations or modifications other than RAC approved kits.
Member of GAMA
General Aviation Manufacturers Association
Raytheon Aircraft
Beech
Hawker